Earthquake Detection & Early Warning via IoT Sensors

Rahul Kumar1, Raj Chaudhary2, Shivang Shekhar3 , Abhishek Kumar4

Sharda University, Greater Noida , India 1,2,3,4

Email: rg9284728@gmail.com1, [heyrajx77@gmail.com2](mailto:heyrajx77@gmail.com2), [shivangshekhar6213@gmail.com3](mailto:shivangshekhar6213@gmail.com3)

[abhishek.kumar11@sharda.ac.in](mailto:abhishek.kumar11@sharda.ac.in)

**Abstract:— To save lives, most nations have put in place EEW (Early Earthquake Warning) Systems. Given that it is difficult to predict where and when a seismic event will occur, early detection is crucial to minimizing damage to infrastructure and human life. Thus, real-time architecture and effective communication are essential. We recommended our system for rural areas because they lack the resources to be earthquake aware because it is very affordable and simple to maintain. Our system is very practical and detects in real time. We install an accelerometer sensor (ADXL 335) on the wall to detect earthquake vibrations when they occur. Arduino computes the data and, if the vibrations are significant, generates an alarm to alert people immediately and direct them to safer places.**

***Index Terms*— Earthquake early warning, Vibrations Sensors, Seismic Sensors Acceleration sensor, Arduino Uno.**

1. **Introduction**

Modern technologies can now be used for real-time monitoring of numerous geological disasters thanks to the development and application of sensor technology[12]. Smart healthcare, intelligent transportation systems, smart buildings, and earthquake early warning systems are just a few of the industries that have seen widespread adoption of cutting-edge computing technologies in recent years. These technologies include wireless networking, Bluetooth, Wi-Fi, and other MEMS (Micro Electro Mechanical Systems) sensors, as well as mobile computing and Internet of Things (IoT) systems. Significant seismic activity is being felt in both the southern and northern regions of Asia. The earthquake that shook Nepal in May 2015 happened on one of the fault lines that connect these[2,10].




Fig.1. Schematic diagram of India-Asia convergent [4 ].

This earthquake detection system locates earthquake vibrations by utilizing Accelerated Sensors, Seismic Sensors (Vibration Sensors), and Generate an Alarm so that people are alerted prior to casualties[14].

|  |
| --- |
| **Descriptor Magnitude Average Annually** |
| Great 8 and higher 1\*  Major 7 – 7.9 17\*  Strong 6 – 6.9 134\*  Moderate 5 – 5.9 1319\*  Light 4 – 4.9 13,000(est.)  Minor 3 – 3.9 130000(est.)  Very Minor 2 – 2.9 1300000(est.) |

Table 1. Global frequency of earthquake by U.S Geological survey [4]

An ATmega328-based microcontroller board called the Arduino Uno. The Arduino Uno has a USB port, a power jack, an ICSP header, a reset button, and a 16 MHz crystal oscillator, 14 input pins for digital output, 6 pins for PWM output, and 6 pins for analogue input. It might be used to couple microcontroller power. USB connections, AC-to-DC power adapters, or batteries can all be used to power an Arduino Uno board when connecting it to a computer. To commemorate the release of Arduino 1.0, the name "Uno," which translates to "one," was chosen. The most recent Arduino USB board, Uno and 1.0 will be utilized as the default Arduino configuration.

The Arduino Uno's power can be started with either a USB connection or an external (automatic) power source[6]. Batteries and AC-to-DC converters are examples of external (non-USB) power sources. By inserting a center-positive plug jack with a 2.1mm size POWER connector, this adapter may be connected. The G and V in header pins on the POWER connection can be used to connect the battery head. The Uno board should operate between 7 and 12 volts, according to the recommended voltage range. The Uno pin 5v can still operate when the power supply is less than 7 volts, but it is unstable. The voltage regulator could overheat and harm the Uno board if more power is drained from the 12V source.

This study explains how the earthquake early warning system behaves over a wide geographic area. An earthquake monitoring system is essential. A natural disaster cannot be completely stopped by humans, but they can analyze it and take significant steps to reduce the damage[9].

**Accelerometer ADXL335**

Prior to an earthquake, the acceleration sensor is incredibly responsive to movement and vibration.[9]The ADXL335 offers complete 3-axis acceleration measurement. It is possible to detect accelerations of up to 3 g in the x, y, and z axes. A polysilicon surface-micro machine sensor and a signal processing circuit make up an accelerometer sensor.

1. **Literature Survey**

Several countries and organizations began adopting MEMS sensors to realize the EEW as seismological theories and signal processing technology developed during the previous few decades. However, the deployment size of these sensors and the network topology of the system are not taken into consideration. Using the EEW requires the ability to deploy sensors and analyze data [7]. In order to achieve higher dimensionality in the spatial and temporal domains, Kenji Nishida et.al. [10] designed a 3-dimensional (3D) convolution architecture for earthquake detection and expanded the use of feature extraction for seismic signals based on logmel spectrograms. In many different applications, including audio-visual recognition, human action detection for video processing, and dynamic gesture recognition tasks, the 3D-CNN architecture is used to model the spatiotemporal information inherited from hierarchical structure[3],[14].

Nishu Pandey et. al. [4] introduced NodeMCU controls the entire software stack on the Arduino Uno. It has an 8-bit RISC processor, a 16 MHz CLK speed, 32 KB of code storage, 2 KB of SRAM, and 1 KB of EEPROM. Without a fixed refrence, MEMS sensors can measure linear motion, movement, shock, or vibration. Sensor data is sent to the cloud using the IOT platform ThingSpeak.

The ADXL335 accelerometer is a part of the early warning system for earthquakes[3]. This accelerometer has a gyroscope, a magnetometer, and a 3-axis capacitive accelerometer that aid in the detection of earthquake-related vibrations. The use of a warning and alarm system is suggested as a productive way to effectively keep track of significant earthquake- and flood-prone areas in real time. A float sensor, which measures the water level, is a component of the system that warns the occupants of the home depending on the strength of the water level [11].

To detect earthquake shocks, the SES60 sensor will be equipped. Findings from the detection are used to create voltage levels. Voltage level is the Arduino board's input. When deciding whether there is vibration, the Arduino selects them after converting the level input to digital data. In the event that Arduino detects an earthquake trembling, the Ethernet Shield module sends the data to the website. Data is kept on the web server in the database. An image of the most recent earthquake and the most recent tremor are displayed in the three sections of the main display on the PC monitor [5].

Khan et al. [8] distinguished between static and dynamic environments for seismic detecting systems, and in the former, they applied the ANN model to evaluate a number of variables. This initial vibration as a signal early warning system to provide alarms and notifications via the Internet. This can be done because the system is based on internet of things.

1. **Background and Motivation**

An effective method of reducing disaster risk and preventing earthquakes is a EW system. Lethal seismic motion can result in fatalities and property damage in densely populated areas[13]. It may be possible to prevent such deaths by using earthquake-resistant structures or an Earthquake Early Warning (EEW) system, which provides seconds to minutes of advance warning in advance, allowing people to move to safe areas or turn off hazardous machinery. This is because typical human structures cannot withstand earthquakes of large magnitude. Building earthquake-resistant buildings is expensive, and it is challenging to create a highly accurate national EEW system. Seismic sensors, also known as vibration sensors, were set up at work to detect earthquakes and generate alarms in an effort to save as many lives as possible.

# Proposed Method

Utilizing accelerometers, it is possible to identify the primary earthquake vibrations along any of the three axes. in light of this, The accelerometer measures vibrations, and it converts those vibrations into corresponding ADC values. Using the 16x2 LCD, Arduino displays these values. Every time the Arduino turns on, vibrations from the environment are sampled in order to calibrate the accelerometer. In order to obtain the real readings, the sample values must then be subtracted from the actual readings. As a result, when it detects vibrations in its natural environment, it won't show notifications.

After determining the actual readings, Arduino compares these numbers to the predetermined minimum and maximum values. If any axis' specified values are greater or less than the predetermined values in either direction, Arduino detects changes to the settings and, if found, activates a buzzer, an LED, and displays the alert status on a 16x2 LCD (positive or negative). The earthquake detector's sensitivity can be changed by modifying the settings in the Arduino code. We use ADXL(335) sensors for our model, and we simply stick the sensors to the wall and connect them to an Arduino Uno. Whenever an earthquake occurs, the vibrations are detected by the accelerometer sensors (i.e., ADXL 335) that are stuck to the wall, and the data is computed on the Arduino Uno if it determines that the vibrations are significant enough to generate an alarm.




Fig.2. Flow Chart of Proposed Earthquake System

1. **Conclusion**

This suggested system primarily relies on accelerator sensors, such as the ADXL 335, which are installed on the house's walls so that they can pick up vibrations clearly. It detects earthquake vibrations and sends the data to the Arduino Uno system, which checks the data to see if it is negligible or not. If the data is significant and it will cause damage or harm to people, it will generate alarms so that people can protect themselves.

**References**

1. Dyane Putriera Anggraenia , Nonoh Siti Aminahb , Yohanes Radiyonoc “ EQUIPMENT OF EARTHQUAKE DETECTION AND WARNING WITH VIBRATION SENSOR”journal ICTTE,Vol 1, Nomor 1, Januari 2016.
2. Pan Xiong 1 , Dedalo Marchetti 2,3 , Angelo De Santis 3 , Xuemin Zhang 1 and Xuhui Shen 4,\*, “SafeNet: SwArm for Earthquake Perturbations Identification Using Deep Learning Networks”, Journal MDPI.
3. Ahmed Shaheen 1,\* , Umair bin Waheed 1 , Michael Fehler 2 , Lubos Sokol 3 and Sherif Hanafy 1, “GroningenNet: Deep Learning for Low-Magnitude Earthquake Detection on a Multi-Level Sensor Network”, MDPI.
4. Nishu Pandey, K. Hari Simha Rao, V. Seshank, Shashank Pokala, Aparna T Sunil, “EARTHQUAKE ALERT SYSTEM BASED ON IOT TECHNOLOGY” journal JETIR, May 2021, Volume 8, Issue 5.
5. Edidas1 , Rusnardi Rahmat Putra2,3, “Designing and building earthquake warning system with Arduino and web-based SES60 SLP sensor”, Journal-Bulletin of Electrical Engineering and Informatics, Vol. 11, No. 1, February 2022, pp. 581~588.
6. Silja Varghese1 , Acksa Varghese2 , Aiswarya Jagadees3 , E. K. Anupriya Vijayan4, “Earthquake Detector Using Arduino, International Journal of Research in Engineering, Science and Management, Volume-3, Issue-4, April-2020.
7. Aming Wu\*, Jangsoo Lee\*, Irshad Khan, Young-Woo Kwon, “CrowdQuake+: Data-driven Earthquake Early Warning via IoT and Deep Learning”,IEEE,2021.
8. Irshad Khan, Seonhwa Choi and Young-Woo Kwon 1,\*, “ Earthquake Detection in a Static and Dynamic Environment Using Supervised Machine Learning and a Novel Feature Extraction Method”,MDPI, 1 February 2020.
9. G Gunawan, B B Nasution , M Zarlis , Marliana Sari1 ,AR Lubis1 and Solikhun2, “ Design of Earthquake Early Warning System Based on Internet of Thing”,ICoCISM journal of Physics,1830 (2021).
10. Muhammad Shakeel1 · Katsutoshi Itoyama1 · Kenji Nishida1 · Kazuhiro Nakadai1,2, “ Detecting earthquakes: a novel deep learning-based approach for effective disaster response”,Springer, 1 April 2021
11. Venita Babu, Dr. Vishnu Rajan, “ FLOOD AND EARTHQUAKE DETECTION AND RESCUE USING IOT TECHNOLOGY ”, IEEE, ICCES 2019.
12. Jangsoo Lee1 , Jae-Seon Kim2 , Seonhwa Choi2 , and Young-Woo Kwon1, “ A Smart Device Using Low-cost Sensors to Detect Earthquakes ”, IEEE,2019.
13. Tai-Lin Chin , Member, IEEE, Chin-Ya Huang, Member, IEEE, Shan-Hsiang Shen, Member, IEEE, You-Cheng Tsai, Yu Hen Hu , Fellow, IEEE, and Yih-Min Wu, “ Learn to Detect: Improving the Accuracy of Earthquake Detection”,IEEE, VOL. 57, NO. 11, NOVEMBER 2019.
14. Zhenyu Bao 1 , Jingyu Zhao 2 , Pu Huang 3,\*, Shanshan Yong 1,4 and Xin’an Wang 1, “ A Deep Learning-Based Electromagnetic Signal for Earthquake Magnitude Prediction ”,MDPI, 28 June 2021.